                          PACKET STATIONS
REV: 06JAN04

PACKET IDENTIFIER
LOCATION

MBARI    
Cupola - OASIS Telemetry

TORO     
Mt. Toro - OASIS Telemetry

XXXXM1*  
M-1 OASIS Telemetry

XXXXM2*   
M-2 OASIS Telemetry

MBARI
Cupola - GPS Diff. & Ships Position

TORO  
Mt. Toro - GPS Diff. & Ships Position

LOBOS  
Pt. Lobos - GPS Diff. & Pt. Lobos Position

FLYER  
Western Flyer - GPS Diff. & Western Flyer Position

ZEPHER
ZEPHER - GPS Diff. & Western Flyer Position

*DEPLOYMENT YEAR

MBARI.SET  Cupola - OASIS Telemetry

Ax25l2v2 
ON

MYcall   
MBARI

REtry    
15

TXUifram 
ON

TORO.SET  Mt. Toro - OASIS Telemetry

Ax25l2v2 
ON

CMSg     
ON

CText    
******** WNWN547 ********

CWid     
EVERY 6

CWIDText 
WNWN547

MYcall   
TORO

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON


PAGE 1/7

OASIS TNC COMMANDS

(commands sent to TNC on initialization in order sent)

NOmode
ON

ECho
OFF

AX2512v2
ON

AUtolf
OFF

BBSmsgs
ON

Paclin 
0

PACTime
After 3

DWait
33

TXDelay
33

FRack
5

MAXFrame
4

CPactime
ON

CR
OFF

Monitor 
0

CONMode
C

SEndpac
$1A

TXUifram
OFF

Flow
OFF

STReamsw
0

ADRdisp
OFF

Mycall*
XXXXMZ

On the shore side the following are used to set up and restore the TNC:

setup_tnc =  NOmode OFF\r, ECho OFF\r, RETry 15\r", CHeck 6\r, Monitor OFF\r"
restore_tnc = ECho ON\r

* X denotes deployment year

  Z denotes morring number
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MBARI_1.SET  Cupola - GPS Diff. & Ships Position

Ax25l2v2 
ON

BReak    
OFF

DATAMode
ON

Echo     
OFF

MAll     
OFF

MCOM     
ON

MFilter  
$0A

Monitor  
ON

MStamp   
ON

MYcall   
MBARI

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
CQ via TORO

TORO_1.SET  Mt. Toro - GPS Diff. & Ships Position

Ax25l2v2 
ON

CMSg     
ON

CText    
******** WNWN547 ********

CWid     
EVERY 6

CWIDText 
WNWN547

MYcall   
TORO

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

LOBOS.SET  
Pt. Lobos - GPS Diff. & Pt. Lobos Position

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode 
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
LOBOS

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO
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FLYER.SET  
Western Flyer - GPS Diff. & Western Flyer Position 

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode 
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
FLYER

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO

ZEPHER.SET  
ZEPHER - GPS Diff. & Western Flyer Position 

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
FLYER

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO
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IDEAS FOR KANTRONICS TNC’s WITHOUT NAVPROC

LOBOS_1.SET  
Pt. Lobos - GPS Diff. & Pt. Lobos Position

REM  
PT LOBOS POS REPORT SETUP

REM 
SET DAytime yymmddhhmmss AFTER PROGRAMING

INT 
TERM

MYcall 
LOBOS

CWId 
WNWN547

CWIDText 
Every 10

GPSPort 
4800 NOrmal NOCHECK

DAYStr 
ddmmmyyyy hhmm.ss ZULU

HEAderline 
OFF

Monitor 
OFF

MCOM 
OFF

MCon 
OFF

MStamp 
ON

HID 
OFF

MYAlias 
%

UIdigi 
%

UIDWait 
OFF

UIFlood 
%

UITrace 
%

BText 
>MBARI UHF DGPS SYSTEM

Unproto
 CQ

Beacon 
E 121

GPShead 1 
$GPGGA

GPSHead 3 
$GPRMC

GPSTime ON 
RMC

LT 3 
!RV POINT LOBOS, BERTHED IN MOSS LANDING, CA

BLT 1 Every 
00:01:00 STart 00:00:00

BLT 2 Every 
00:29:00 STart 00:00:30

LTP 1 
MBARI

LTP 2 
MBARI

LTP 3 
MBARI

LTP 4 
MBARI
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FLYER_1.SET  
Western Flyer - GPS Diff. & Western Flyer Position 

REM 
WESTERN FLYER POS REPORT SETUP

REM 
SET DAytime yymmddhhmmss AFTER PROGRAMING

INT 
TERM

MYcall 
FLYER

CWId 
WNWN547

CWIDText 
Every 10

GPSPort 
4800 NOrmal NOCHECK

DAYStr 
ddmmmyyyy hhmm.ss ZULU

HEAderline 
OFF

Monitor 
OFF

MCOM 
OFF

MCon 
OFF

MStamp 
ON

HID 
OFF

MYAlias 
%

UIdigi 
%

UIDWait 
OFF

UIFlood 
%

UITrace 
%

BText 
>MBARI UHF DGPS SYSTEM

Unproto 
CQ

Beacon 
E 121

GPShead 1 
$GPGGA

GPSHead 3 
$GPRMC

GPSTime 
ON RMC

LT 2 
!RV WESTERN FLYER BERTHED IN MOSS LANDING, CA

BLT 1 
Every 00:01:00 STart 00:00:20

BLT 2 
Every 00:30:00 STart 00:00:30

LTP 1 
MBARI

LTP 2 
MBARI

LTP 3 
MBARI

LTP 4 
MBARI
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ZEPHER.SET  
ZEPHER - GPS Diff. & Western Flyer Position

REM 
ZEPHER POS REPORT SETUP

REM 
SET DAytime yymmddhhmmss AFTER REM PROGRAMING

INT 
TERM

MYcall 
ZEPHER

CWId 
WNWN547

CWIDText 
Every 10

GPSPort 
4800 NOrmal NOCHECK

DAYStr 
ddmmmyyyy hhmm.ss ZULU

HEAderline 
OFF

Monitor 
OFF

MCOM 
OFF

MCon 
OFF

MStamp 
ON

HID 
OFF

MYAlias 
%

UIdigi 
%

UIDWait 
OFF

UIFlood 
%

UITrace 
%

BText 
>MBARI UHF DGPS SYSTEM

Unproto 
CQ

Beacon 
E 121

GPShead 1 
$GPGGA

GPSHead 3 
$GPRMC

GPSTime 
ON RMC

LT 2 
!RV ZEPHER, BERTHED IN MOSS LANDING, CA

BLT 1 
Every 00:01:00 STart 00:00:40

BLT 2 
Every 00:31:00 STart 00:00:30

LTP 1 
MBARI

LTP 2 
MBARI

LTP 3 
MBARI

LTP 4 
MBARI
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