cript started on Tue Mar 24 10:40:41 1998

orca:/users/teto[31]> rlogin entropy -l pcdisk

Please wait...checking for disk quotas

        ***********************************************************

           ######  #    #   #####  #####    ####   #####    #   #

           #       ##   #     #    #    #  #    #  #    #    # #

           #####   # #  #     #    #    #  #    #  #    #     #

           #       #  # #     #    #####   #    #  #####      #

                    Welcome to HP-UX on the HP 9000 Series

                   Monterey Bay Aquarium Research Institute

                  HP-UX entropy A.09.04 E 9000/887 931751281

        ***********************************************************

[1] % cd /usr/troll

[3] % ./wf-seatel 

This is the program to connect to the Smart Switch at the MCOE site on Mt Toro.

P shows AZ/EL, Axxxx sets AZ, Exxxx sets EL.

Bxxxx sets Heading, M views tracking parameters.

% shows signal strength (AGC), should be in the Dxx range.

Typing any of the above control characters without input will result in a 0 being implied.

When exiting the Seatels in is important to type Cntrl-B 0 E. Other characters may spoof the Seatel

Type ESC Cntrl-B 0 B to get to the PL Seatel.

Elevation 000 seems to be the right number. 

Heading should be 312.5  (check with H)

Tracking parameters should be N040 Y000 X001 (check with M)

Signal strength should be in the DXX range.

Type ESC Cntrl-B 0 C to get to the WF Seatel.

Elevation 000 seems to be the right number. 

Heading should be 312.5  (check with H)

Tracking parameters should be N040 Y000 X001 (check with M)

Signal strength should be in the DXX range

Type ESC Cntrl-B 0 D to get to the DGPS digipeater.

Type ESC Cntrl-B 0 E to get to the Knox switch.

Type ESC Cntrl-B 0 F to get to the Magni video generator

Type ESC Cntrl-B 0 A to get to the loopback.

Connecting thru wf-seatel.port, speed 9600.

The escape character is CTRL-\ (28).

[Back at Local System]

[4] % logout

Connection closed.

script done on Tue Mar 24 10:41:40 1998

