                          PACKET STATIONS
REV: 11JUL03

PACKET IDENTIFIER
LOCATION

MBARI    
Cupola - OASIS Telemetry

TORO     
Mt. Toro - OASIS Telemetry

XXXXM1*  
M-1 OASIS Telemetry

XXXXM2*   
M-2 OASIS Telemetry

MBARI
Cupola - GPS Diff. & Ships Position

TORO  
Mt. Toro - GPS Diff. & Ships Position

LOBOS  
Pt. Lobos - GPS Diff. & Pt. Lobos Position

FLYER  
Western Flyer - GPS Diff. & Western Flyer Position

ZEPHER
ZEPHER - GPS Diff. & Western Flyer Position

*DEPLOYMENT YEAR

MBARI.SET  Cupola - OASIS Telemetry

Ax25l2v2 
ON

MYcall   
MBARI

REtry    
15

TXUifram 
ON

TORO.SET  Mt. Toro - OASIS Telemetry

Ax25l2v2 
ON

CMSg     
ON

CText    
******** WNWN547 ********

CWid     
EVERY 6

CWIDText 
WNWN547

MYcall   
TORO

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON
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OASIS TNC COMMANDS

(commands sent to TNC on initialization in order sent)

NOmode
ON

ECho
OFF

AX2512v2
ON

AUtolf
OFF

BBSmsgs
ON

Paclin 
0

PACTime
After 3

DWait
33

TXDelay
33

FRack
5

MAXFrame
4

CPactime
ON

CR
OFF

Monitor 
0

CONMode
C

SEndpac
$1A

TXUifram
OFF

Flow
OFF

STReamsw
0

ADRdisp
OFF

Mycall*
XXXXMZ

On the shore side the following are used to set up and restore the TNC:

setup_tnc =  NOmode OFF\r, ECho OFF\r, RETry 15\r", CHeck 6\r, Monitor OFF\r"
restore_tnc = ECho ON\r

* X denotes deployment year

  Z denotes morring number
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MBARI_1.SET  Cupola - GPS Diff. & Ships Position

Ax25l2v2 
ON

BReak    
OFF

DATAMode
ON

Echo     
OFF

MAll     
OFF

MCOM     
ON

MFilter  
$0A

Monitor  
ON

MStamp   
ON

MYcall   
MBARI

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
CQ via TORO

TORO_1.SET  Mt. Toro - GPS Diff. & Ships Position

Ax25l2v2 
ON

CMSg     
ON

CText    
******** WNWN547 ********

CWid     
EVERY 6

CWIDText 
WNWN547

MYcall   
TORO

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

LOBOS.SET  
Pt. Lobos - GPS Diff. & Pt. Lobos Position

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode 
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
LOBOS

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO
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FLYER.SET  
Western Flyer - GPS Diff. & Western Flyer Position 

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode 
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
FLYER

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO

ZEPHER.SET  
ZEPHER - GPS Diff. & Western Flyer Position 

ADrdisp  
OFF

Ax25l2v2 
ON

BReak    
OFF

DATAMode
ON

Echo     
OFF

MAll     
OFF

Monitor  
ON

MYcall   
FLYER

NEwmode  
OFF

REMoteio 
ON

STReamsw 
$00

TXUifram 
ON

Unproto  
MBARI VIA TORO
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