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UHF PACKET RADIO/TNC TRAVELER

RADIO
K44GNF1001A

S/N
163FVA0126L

TNC
UMPAD

S/N
2124


SPEC
MEAS
DATE
                      COMMENTS

FREQ
461.7875
461.7872
24OCT2002
UNIT WAS REMOVED FROM 2001M1

PO
2W
2W
24OCT2002
TNC REQUIRES KEY PIN REMOVED

ITX
1.6A
1.16A
24OCT2002


DEV
±3 KHz
±3 KHz
24OCT2002


SINAD
>-112 dBm
-115 dBm
24OCT2002
CONNECTED WITH RFLAB TNC AND PASSED 

IRX
<120 ma
90 ma
24OCT2002
DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN TO “RFLAB”



1ST SOFTWARE CONN TO “RFLAB”



2ND SOFTWARE CONN TO “RFLAB”



1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



IN BAR

1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”
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