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UHF PACKET RADIO/TNC TRAVELER

RADIO
450S

S/N
10445A039A 13917

TNC
UMPAD

S/N
U0702


SPEC
MEAS
DATE
                      COMMENTS

FREQ
461.7875
461.7872
07JAN2003
TNC REQUIRES KEY PIN REMOVED

PO
2W
2W
07JAN2003


ITX
1.6A
1.18A
07JAN2003


DEV
±3 KHz
±3 KHz
07JAN2003


SINAD
>-112 dBm
-114 dBm
07JAN2003


IRX
<120 ma
104 ma
07JAN2003
CONNECTED WITH RFLAB TNC AND PASSED DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN TO “RFLAB”



1ST SOFTWARE CONN TO “RFLAB”



2ND SOFTWARE CONN TO “RFLAB”



1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



IN BAR

1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”
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