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UHF PACKET RADIO/TNC TRAVELER

RADIO
450S

S/N
13919

TNC
UMPAD

S/N
U1832


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
461.7875
29MAY03


PO
2W
2W
29MAY03


ITX
<1.60A
1.13A
29MAY03


DEV
±3 KHz
±3 KHz
29MAY03


SINAD
>-112 dBm
-114 dBm
29MAY03


IRX
<120 ma
108ma
29MAY03


BENCH TEST
PASS
29MAY03
CONNECTED WITH RFLAB TNC AND PASSED DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “RFLAB”



2ND SOFTWARE CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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