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UHF PACKET RADIO/TNC TRAVELER

RADIO
450S

S/N
13919

TNC
UMPAD

S/N
U2013


SPEC
MEAS
DATE
                      COMMENTS

FREQ
461.7875
461.7877
09SEPT03


PO
2W
2W
09SEPT03


ITX
1.6A
1.17A
09SEPT03


DEV
±3 KHz
±3 KHz
09SEPT03


SINAD
>-112 dBm
-116 dBm
09SEPT03
CONNECTED WITH RFLAB TNC AND PASSED 

IRX
<120 ma
92 ma
09SEPT03
DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN TO “RFLAB”



1ST SOFTWARE CONN TO “RFLAB”



2ND SOFTWARE CONN TO “RFLAB”



1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



IN BAR

1ST SOFTWARE CONN TO “TORO”



2ND SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN TO “TORO”



FINAL SOFTWARE CONN TO “TORO”
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