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UHF PACKET RADIO/TNC TRAVELER

RADIO
RNET 450S

S/N
13920

TNC
UMPAD

S/N
U1140


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
461.7875
16JUL02


PO
2W
2W
16JUL02


ITX
<1.60A
.88A
16JUL02


DEV
±3 KHz
±3 KHz
16JUL02


SINAD
>-112 dBm
-115 dBM
16JUL02


IRX
<120 ma
102 ma
16JUL02


BENCH TEST
CONN WITH TORO
16JUL02
ONE WEEK BENCH TEST

    CAN #




  MOORING
2002M1



IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “RFLAB”



2ND SOFTWARE CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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