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UHF PACKET RADIO/TNC TRAVELER

RADIO
K44GNF1001A

S/N
163FSY3470L

TNC
UMPAD

S/N
U1830


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7625
461.7627
28/06/02
NOTE FREQUENCY

PO
2W
3.4W
28/06/02


ITX
<1.60A
1.15A
28/06/02


DEV
±3 KHz
±3 KHz
28/06/02


SINAD
>-112 dBm
-115 dBm
28/06/02


IRX
<120 ma
105 ma
28/06/02


BENCH TEST
PASS
01/07/02
CONNECTED WITH RFLAB TNC AND PASSED DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “RFLAB”



2ND SOFTWARE CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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