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UHF PACKET RADIO/TNC TRAVELER

RADIO
K44GNF1001A

S/N
163FSY3470L

TNC
UMPAD

S/N
U0406


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
461.7876
09JUN03


PO
2W
2W
09JUN03


ITX
<1.60A
1.13A
09JUN03


DEV
±3 KHz
±3 KHz
09JUN03


SINAD
>-112 dBm
-116 dBm
09JUN03


IRX
<120 ma
105 ma
09JUN03


BENCH TEST
PASS
09JUN03
CONNECTED WITH RFLAB TNC AND PASSED DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “RFLAB”



2ND SOFTWARE CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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