
[image: image1.png]uuuuu




OASIS MOORING 
     [image: image2.png]




UHF PACKET RADIO/TNC TRAVELER

RADIO
K44GNF1001A

S/N
163FSY4536L

TNC
UMPAD

S/N
U2126


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
461.7875
07JAN03


PO
2W
2W
07JAN03


ITX
<1.60A
1.15A
07JAN03


DEV
±3 KHz
±3 KHz
07JAN03


SINAD
>-112 dBm
-112 dBm
07JAN03


IRX
<120 ma
107 ma
07JAN03


BENCH TEST
PASS
14JAN03
CONNECTED WITH RFLAB TNC AND PASSED DATA

    CAN #




  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “RFLAB”



2ND SOFTWARE CONN WITH “RFLAB”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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