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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SN

S/N
16946 - N


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
466.78750
466.78755
21SEPT04
RADIO TYPE: 3412  S/N: 29061

PO
2.5W
2.5W
21SEPT04
FIRMWARE: rev4.43  BOARD: rev1.02

ITX
<1.60A
1.49 A
21SEPT04


DEV
±3 KHz
±3 KHz
21SEPT04


RSENS
>-105 dBm
-110 dBm
21SEPT04


IRX
<200 ma
170 ma
21SEPT04
CW ID ON

BENCH TEST
PASS
21SEPT04
#101 OF GRP 1 – DEST ADDR #1 OF GRP 1

    CAN #
N/A
21SEPT04
TO BE DEPLOYED AT MT TORO – 2004M1T

  MOORING
2004M1



IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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