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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SS

S/N
17021 - SMA


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
461.7875
18MAR04


PO
2.5W
2.5W
18MAR04


ITX
<1.00A
615 ma
18MAR04


RSENS
>-103 dBm
-110 dBm
18MAR04


IRX
<160 ma
157 ma
18MAR04


BENCH TEST
PASS
18MAR04
#1 OF GRP 1 – DEST ADDR #2 OF GRP 1

    CAN #

18MAR04
2004M2

  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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