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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SS

S/N
18325 - SMA


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
466.7875
466.7877
26OCT04
RADIO TYPE: 3412  S/N: 34238

PO
2.5W
2.5W
26OCT04
FIRMWARE: rev4.75  BOARD: rev1.05

ITX
<2.00A
1.31 A
26OCT04
UPGRADED FIRMWARE

DEV
±3 KHz
±3 KHz
26OCT04


RSENS
>-105 dBm
-110 dBm
26OCT04


IRX
<200 ma
168 ma
26OCT04
CONFIG FILE: 2004M1A

BENCH TEST
PASS
26OCT04
#4 OF GRP 4 – DEST ADDR #104 OF GRP 4

    CAN #

26OCT04
2004M1 – REPLACE SN 16912 IN FIELD

  MOORING
2004M1



IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”
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