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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SN

S/N
18357 - N


SPEC
MEAS
DATE
                      COMMENTS

FREQ 1
461.7625
461.7628
28APR05
CLEAR CHAN SCAN – TWO FREQS

FREQ 2
461.7875
461.7879


28APR05
FIRMWARE: REV: 4.79  BOARD: REV: 1.05 

S/N: 18357

PO
5W
5W


28APR05
RADIO TYPE: 3412  S/N: 34669

ITX
<2.20A

@12.5VDC
1.82 A

@12.5VDC
28APR05


DEV
±3 KHz
±3 KHz


28APR05


RSENS
>-105 dBm
-110 dBm


28APR05


IRX
<200 ma

@12.5VDC
175 ma

@12.5VDC
28APR05


BENCH TEST
PASS
28APR05


    CAN #
N/A



  MOORING


INSTALLED ON MT TORO

IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH 

 “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



 FINAL SOFTWARE CONN WITH   

 “TORO”
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