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UHF TELEDESIGN RADIO TRAVELER

RADIO
TS4000A05B45SS

S/N
22849 - SMA


SPEC
MEAS
DATE
                      COMMENTS

FREQ 
461.7875
466.7881
05NOV04
RADIO TYPE: 3412  S/N: 37669

PO
2.5W
2.5W
05NOV04
FIRMWARE: rev4.76  BOARD: rev1.06 S/N: 22849

ITX
<1.60A
1.27 A
05NOV04


DEV
±3 KHz
±3 KHz
05NOV04


RSENS
>-105 dBm
-110 dBm
05NOV04


IRX
<200 ma
167 ma
05NOV04
2004M2 REPLACEMENT

BENCH TEST
PASS
05NOV04


    CAN #
N/A



  MOORING




IN OASIS LAB

INSTALL IN CAN



VISUAL INSPECTION



INITIAL CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



IN BAR

1ST SOFTWARE CONN WITH “TORO”



2ND SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ON DEPLOYENT VESSEL

1ST SOFTWARE CONN WITH “TORO”



FINAL SOFTWARE CONN WITH “TORO”



ACCEPTANCE BY MOORING MASTER

NAME: 

TITLE: 

DATE: 


