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Do Not Read

Important Information about Programming Radio Frequencies into the TS4000 Radio Modem

The TS4000 configuration software shipped with your order of TS4000 radio modems allows you to modify the configuration of the radio modems from their factory defaults.   In order to allow our Dealers and OEM customers to program new channel frequencies into the radio modems, a password must be entered into the configuration software.  

To enable channel frequency programming, open the TS4000 configuration software, then open the “Modem Configuration” menu, click on the “Window” pull down menu, and then select “Enable Options…”.  In the password box that opens on the screen, enter “FREQ” (all caps) and choose “OK”.  The channel frequency programming menu will now allow you to program new frequencies into the radio in addition to displaying what is currently programmed.

To enable test mode, open the TS4000 configuration software, then open the “Modem Configuration” menu, click on the “Window” pull down menu, and then select “Enable Options…”.  In the password box that opens on the screen, enter “TEST” (all caps) and choose “OK”.  The test menu will now allow you to test various modes of the radio.
