Jose Rosal
MBARI

7700 Sandholdt Road

Moss Landing, CA 95039

Subject: Parts for MBARI’s CIS/CIP database
Capacitors:

· Tantalums

· AVX Corp General size

· TAJ & TAC

· 22, 47, 10 (All decade values)

· 6.3V, 16V, 25V (voltage ranges)

· AVX Corp Low ESR size

· TPS & TCJ

· 22, 47, 10 (All decade values)

· 6.3V, 16V, 25V (voltage ranges)

· Ceramics

· Kemet Ceramic Chip Standard C0G (NPO)

· C****C***J*GAC
· 22, 47, 10 (All decade values)

· 16V-100V (voltage ranges)

· 5%

· 0603, 0805, 1206

· Kemet Ceramic Chip Standard X7R

· C****C***K*RAC

· 22, 47, 10 (All decade values)

· 16V-100V (voltage ranges)

· 10%

· 0603, 0805, 1206

· Aluminum Electrolytics

· United Chemi-Con Aluminum Electrolytics (SMD)

· All available PXS series values

· All available MVE series values

Resistors

· Chip Resistors

· Vishay/Dale

· CRCW Series

· 0603, 0805, 1206

· All EIA 1% values

· All EIA 5% values
Test Points

· Keystone Electronics
· 5015

· THM Series

Connectors

· Hirose

· PCN10 Series DIN
· 2/3 Rows

· 20, 32, 44, 50, 64 contacts

· Male/female

· Vertical/Right Angle

· Molex

· 70553 Series

· 2-15 positions

· 70543 Series

· 2-15 positions

· 50-57-94** Series

· 2-15 positions

· Samtec

· TSW Series

· 0.100” Centers

· Single Row 1-12 contacts

· Dual Row 4-24 contacts

· -07 Lead Style
· -F Plating Option

· Phoenix Contact

· MC 0,5/**-G-2,5 series (Header)
· MC 1,5/**-G-3,81 series (Header)
· MC 1,5/**-G-5,08 series (Header)
· EMC 0,5/**-G-2,5 series (R/A Header)

· EMC 1,5/**-G-3,81 series (R/A Header)

· EMC 1,5/**-G-5,08 series (R/A Header)

· MC 1,5/**-ST-3,81 series (Plug)

· MC 1,5/**-ST-5,08 series (Plug)

* = fill in value
