Intall OrCAD 17.4 software:
1. Go to the following link and run Setup.exe to install OrCAD Base Release: \\atlas\projectLibrary\TechServices\Software\ORCAD_UPDATES\Cadence_17-4\BaseRelease\Base_SPB17.40.000_wint_1of2
2. 

Open Cadence download manager: Start>Cadence>Download Manager
1. Log into your Cadence account.
a. If you already have an account already set up with Cadence skip to step 2 Update.
b. If you don’t have an account with Cadence…
i. 
2. Update OrCAD 17.4
a. On the left tab click “OrCAD/Allegro”
b. Find “Cadence OrCAD and Allegro 17.4-2019” and click update.
c. Follow the install prompts and complete the update.
3. Install CIP
a. On the left tab click “CIP”
b. Find “OrCAD CIP Client (17.4)” and click “Get”
c. Path to CIP web interface is… \\water2\cip-e
d. 
4. Install EDM
a. On the left tab click “EDM”
b. Find “OrCAD EDM Client (17.4)” and click “Get”
c. Path to EDM web interface is:  \\water2\edm
d. 
e. 
[bookmark: _GoBack]
