EDM Install:
1. Make sure you are running the latest version of OrCAD before installing the EDM Client software.  Go to the following address to run the OrCAD updater: \\atlas\ProjectLibrary\TechServices\Software\ORCAD_UPDATES\Cadence_17-4\HF_018
[bookmark: _GoBack]
2. Run the EDA Client EXE in from the following location: \\atlas\ProjectLibrary\TechServices\Software\ORCAD_UPDATES\EDM174\EDM1740P1\HF_014 
a. The installation home screen will open
b. Click Next
c. [image: ]
d. Use the default destination location. Click Next.[image: ]
e. Select where you want your shortcuts if any then click Next.[image: ]
f. For the EDM URL enter: http://water2/edm then click Next.[image: ]
g. Click Install
 [image: ]
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