Option 1:
	Color 
	Designation 

	Black 
	Power Common, Return, Ground

	Brown 
	Signal Ground, 485/232 Common

	Red 
	Primary Logic Power

	Orange 
	+12Vdc, +15Vdc 

	Yellow 
	+48Vdc 

	Green 
	Chassis / Frame 

	Blue 
	-5Vdc, -12Vdc, -15Vdc

	Violet 
	+24Vdc, +27Vdc

	Grey 
	+36Vdc

	White 
	Secondary Power Common, Return, Ground

	Green/White Stripe
	Sea Water Ground (18 AWG)

	White/Brown Stripe 
	MISC 24-20AWG wire / Misc Signal 1

	White/Red Stripe 
	MISC 24-20AWG wire / Misc Signal 2 / 
Secondary Logic Power

	White/Orange Stripe 
	MISC 24-20AWG wire / Misc Signal 3

	White/Yellow Stripe 
	MISC 24-20AWG wire / Misc Signal 4

	White/Green Stripe 
	MISC 24-20AWG wire / Misc Signal 5

	White/Blue Stripe 
	MISC 24-20AWG wire / Misc Signal 6

	White/Violet Stripe 
	MISC 24-20AWG wire / Misc Signal 7

	White/Grey Stripe 
	MISC 24-20AWG wire / Misc Signal 8

	White/Black Stripe 
	MISC 24-20AWG wire / Misc Signal 9

	Black/White Stripe
	MISC 24-20AWG wire / Misc Signal 10

	Red/Yellow Stripe
	Primary High Voltage (18AWG - 22AWG)

	Red/Green Stripe
	Secondary High Voltage (18AWG)



Communication (Wires twisted with these color combinations will represent the following)
	Color 
	Designation 
	Color 
	Designation 

	White/Black Stripe 
	485A
	White/Green Stripe 
	Tx 

	White/Brown Stripe
	485B
	White/Blue Stripe
	Rx 

	Brown
	485 Common
	Brown
	232 Common




Pin to Pin Wiring (Option 2)
	Color 
	Designation 

	Brown 
	1

	Red 
	2

	Orange 
	3

	Yellow 
	4

	Green 
	5

	Blue 
	6

	Violet 
	7

	Grey 
	8

	White 
	9

	Black
	10

	White/Brown Stripe 
	11

	White/Red Stripe 
	12

	White/Orange Stripe 
	13 

	White/Yellow Stripe 
	14 

	White/Green Stripe 
	15

	White/Blue Stripe 
	16

	White/Violet Stripe 
	17

	White/Grey Stripe 
	18 

	White/Black Stripe
	19

	Black/White Stripe
	20



