ESP Electro-Mechanical Cable Test Results

Technician:__________________________
Date:_______________________________
Cable:______________________________

1:  Check continuity between pins and mechanical parts.

2:  Hi-Pot Test 150V @ 30secs
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AFTER SOAKING
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