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ATI Wah Chang – Pattern Policy
1. Patterns produced by ATI Wah Chang and invoiced to the Buyer become Buyer’s property.

2. Buyer’s patterns will be stored by ATI Wah Chang for a reasonable length of time pending repeat orders, five (5) years maximum.

3. ATI Wah Chang is not responsible for loss of or damage to pattern equipment by fire or other casualties beyond its control.

4. Buyer supplied pattern and core box equipment should be in proper condition to produce the quantity and quality of castings agreed upon. All repairs and changes necessary to place equipment in proper condition shall be the Buyer’s obligation.
5. ATI Wah Chang reserves the right to mark patterns inconspicuously with its trademark in order that the origin of the casting may be known.

6. ATI Wah Chang will produce castings true to Buyer furnished patterns less the normal pattern shrinkage allowances, but cannot guarantee dimensional tolerances on castings made from these patterns.

7. All duty, bonds and penalties of patterns imported into the U.S. from foreign countries will be the sole responsibility of the Buyer.

8. ATI Wah Chang reserves the right to revise prices quoted on using Buyer furnished patterns if upon receipt and inspection of same it is found that their use involves significant costs not predictable from the pattern description.

9. ATI Wah Chang is not responsible for variations existing between blueprints and pattern and core box equipment supplied by Buyer. If requested by Buyer, ATI Wah Chang will check patterns and core box equipment with blueprints at Buyer’s expense unless otherwise agreed to by ATI Wah Chang.

10. All patterns, core boxes and loose pieces thereof, shall be marked properly for identification.
11. All freight, drayage, boxing and crating charges on patterns, both to and from ATI Wah Chang, shall be assumed by Buyer.

12. When new patterns are to be made, it is recommended that the work be done by an ATI Wah Chang approved vendor so that the best methods for casting the reactive metals may be incorporated into the construction of the pattern equipment.
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