900719_FOCE : xFOCE - Phytec LPC3250 - Install LTIB Linux Build Tools This page last changed on Aug 16, 2012 by headley. LTIB is an alternative to ELDK for configuring Linux kernels for Phytec. LTIB is used to generate the kernel (uImage), u-boot (u-boot.bin) and rootfs (rootfs.tgz) images. =================== Install LTIB =================== - install cvs sudo apt-get install cvs sudo apt-get install g++ sudo apt-get install tcl8.5 sudo apt-get install zlib1g-dev rpm rpm-build ncurses-dev m4 bison perl -MCPAN -e 'install HTTP::Request::Common' sudo cpan cpan> install LWP::UserAgent perl -MCPAN -e 'install LWP::UserAgent' - install LTIB via CVS $ cvs -z3 -d:pserver:anonymous@cvs.savannah.nongnu.org:/sources/ltib co -P ltib $ cd ltib $ ./ltib

Document generated by Confluence on Feb 03, 2026 14:29