900719_FOCE : FOCE PCI-104 Health Monitor This page last changed on Apr 18, 2008 by chadillac. # General Description The HM-PCI104 is a compact board design to monitor the overall health of a PCI/104 stack. It can simultaneously monitor five internal analog voltage inputs, four external analog voltage inputs, one on board temperature sensor, 2 external temperature sensors and 2 fan tachometer inputs. It has pulse width modulation outputs to control the speed rotation of two fans. The HM-PCI104 also provides visual and audio warning when any measurement goes out of a programmable range. # Links Technical Manual Attachments: hmpci104.gif (image/gif) Comments:
Oops. It looks to me like this won't fit into our stack. It uses only the PCI connector and doesn't pass through the ISA connector. So if we put it between the "Plus" and "non-Plus" boards, the ISA bus doesn't get passed through. But we can't put it below the "non-Plus" boards either, because they have no PCI connector to attach this to. Posted by bobh at Apr 01, 2008 09:57

Document generated by Confluence on Feb 03, 2026 14:29