900719_FOCE : Disk Recovery after foce3 mishap This page last changed on Oct 09, 2008 by bobh. #### Recovery Hard disk was still functional! I put it onto the foce2 system in the software lab, and booted it. Borrowed an Acronis TrueImage bootable backup CD from Todd Ruston in IS. Booted off the USB DVD drive, and imaged the entire disk Put this image in //tornado/ProjectLibrary/900719_FOCE/FOCE.Software/foce3Image/foce3.tib I then replaced the foce2 hard disk on this system, and attached the foce3 hard disk as a slave IDE drive. I tar'd the entire foce3 root file system, and placed this tar.gz file into //tornado/ProjectLibrary/900719_FOCE/FOCE.Software/foce3Image/foce3.tar.gz I unmounted the slave drive, and ran e2fsck on it. It passed with flying colors. #### Partition Information for Linux hard disk /dev/hda1 (bootable) Start 1 End 19278 Blocks 154850503 ID 83 Linux /dev/hda2 Start 19279 End 19457 Blocks 1437817 ID 5 Extended /dev/hda5 Start 19279 End 19457 Blocks 1437786 ID 82 Linux swap #### Network Problems If the system doesn't find eth0, you may have a problem with udev mapping, due to using an ethernet adapter with a different MAC address. If this is the case, you must manually edit the file at /etc/udev/rules.d/z25-persistent-net.rules

Document generated by Confluence on Feb 03, 2026 14:29