Oasis Support Engineering : M1 February 2012 This page last changed on Feb 03, 2012 by kgomes. This document details the notes associated with the M1 Mooring turn for October 2011. ##### Schedule
Milestone | Date
--- | ---
Initial Configuration | 7/7
Final Science Instrument list | 7/15
Instruments Due | 7/29
Oasis Software development | 7/18 - 8/9
Buoy Mechanical modifications | 7/18 - 8/9
Oasis Code Freeze | 8/10
System Testing | 8/11 - 8/24
Sensor installation | 8/25 - 9/20
Dockside Testing | 9/21- 26
Load on Pt Sur | 9/27
Deployment and Recovery | 9/28
##### Sensor Listing Here is a Word Doc that details the sensors to be deployed on the M1 Mooring in October. I converted that to a table here:
SENSOR | SERIAL NO | SSDS | LOCATION
--- | --- | --- | ---
Oasis-3 |  |  | tower
E-meter | 041342 | 1602 | tower
Grnd fault | 2 | 1403 | tower
GPS | 80721087 | 1468 | tower
Radio (Viper?) |  |  | tower
Metsys | 1 | 1397 | tower
Windbird | 8 |  | tower
Sonic | A224007 |  | tower
AT/RH | 93250 |  | tower
AsimetLWR | 305 | 1251 | tower
AsimetSWR | 338 | 1250 | tower
HyperOCR | 229 | 1450 | tower
WETStar | 236 | 1425 | tower
pCO2 | IRG2-154 | 1743 | tower
EK-60 |  |  | tower
ISUS | N/A | 1678 | elevator
MicroCAT | 3424 | 1358 | elevator
ADCP | 1384 | 1352 | elevator
ADCPpower | 010 |  | elevator
HydroScat | H2010336 | 1390 | elevator
HSshutter | SS031014 |  | elevator
Pump (fluor) | 52578 |  | elevator
Optode | 131 | 1552 | elevator
pH (self-contained) |  |  | elevator
MicroCAT | 3531 | 1314 | 10m cage
HyperOCR-Ed | 228 | 1451 | 10m cage
Bioshutter | 063 |  | 10m cage
HyperOCR-Lu | 203 | 1452 | 10m cage
Bioshutter | 064 |  | 10m cage
EK-60 transducer |  |  | 10m cage
MicroCAT | 3777 | 1356 | 20m cage
HyperOCR-Ed | 295 | 1625 | 20m cage
Bioshutter | 094 |  | 20m cage
HyperOCR-Lu | 254 | 1627 | 20m cage
Bioshutter | 096 |  | 20m cage
HydroScat-2 | H2061255 | 1629 | 215m nilspin
UIM | 0067 | 1489 | 215m nilspin
ECO-FLNTUSB | 237 | 1470 | 215m nilspin
Deep O2 |  |  | 215m nilspin
SBE-37-IM at 40 |  |  |
SBE-37-IM at 60p |  |  |
SBE-37-IM at 80 |  |  |
SBE-37-IM at 100p |  |  |
SBE-37-IM at 150 |  |  |
SBE-37-IM at 200p |  |  |
SBE-37-IM at 250 |  |  |
SBE-37-IM at 300p |  |  |
Attachments: 2011-M1 Sensor.doc (application/msword) Comments:
Oasis cfg file and app are in CVS at http://moonjelly.shore.mbari.org/cgi-bin/viewvc.cgi/oasis3/deployments/2012M1/ Posted by rich at Apr 16, 2012 13:52

Document generated by Confluence on Feb 04, 2026 08:35