OASIS Turn Instructions for M1 & M2 On Tsunami
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(Revised 29-Apr-2009 )
Begin this after the last download before they release the anchor (eg. after 9am.)
Login as user: oasisa 

cd to /oasis
Turn off downloads
crontab –r
verify with crontab –l

use df or bdf to see if you have enough space for the archive

(2008M2 required about 1.3Gb to archive)
Archive old deployment, setup new 
cd to /oasis/bin/util

Execute one of the following: 
WARNINGS: substitute starting month&year of deployment just ENDING and
the instrument list is for the NEW deployment, (not the one ending!!)
FOR M1 ONLY  (eg. recovering the 2007M1, and deploying 2008M1)
/oasis/bin/util/deployMoor m1 oct2008 aanderaaO2 adcp emeter fluor gps hr1 hr2 hr3 hrh hs2 hyperOCR imhs2 isus lwr metsys microcat microcat2 microcat3 o3gf pco2 swr tstring gpsclock netcdf
FOR M2 ONLY (eg. recovering 2008M2 and deploying 2009M2)
/oasis/bin/util/deployMoor m2 apr2008 aanderaaO2 adcp emeter fluor gps hr1 hr2 hr3 hrh hs2 imhs2 isus lwr metsys microcat microcat2 microcat3 o3gf pco2 swr tstring gpsclock netcdf
Note: will pause a few minute (~3-4) on ‘Processing current data”
Note: may complain awk cant find dir for each instrument (eg adcp/2009) because of ‘process’. Just ignore those error messages. – (this didn’t happen for 2009M2 turn, I think this happened before because I correctly substituted the startdate for the deployment going out, not the one coming in…and we had to correct it manually later).
(FUTURE TODO: should create these dirs in advance and disable that portion of deployMoor…)

Update Header Files using files from test (the above script deleted old cfg and header files)

cp /oasis/test/cfg/m2/* /oasis/cfg/m2
Replace m1.cfg or m2.cfg from test
cp /oasis/test/cfg/m1.cfg /oasis/cfg

vi /oasis/cfg/m1.cfg

· change path in any lines from /oasis/test to /oasis

· resave and exit
Update getM1 (or getM2)

cp /oasis/test/bin/getM1 /oasis/bin

vi /oasis/bin/getM1
· change path in line ~19 from /oasis/test to /oasis
· make sure failmail message subject doesn’t say ‘TEST M?’  (MAIL_MSG near line 85)
· check failmail delivery list.
· check radio IP and port # set correctly

· resave and exit
Reset oasis.rcd
We will delete rcd history for mooring just being recovered and then replace with the list for the can that has been running on the dock. Be careful not to clobber the rcd for any other moorings m1 or m2 still out there ! 
cd /oasis/raw

cp –p oasis.rcd oasis.rdc.foo  (ie. make a safety copy in case you blow the editing below.) 

vi oasis.rcd

- delete any entries for m1.

- move to end of file, add blank line
- :r /oasis/test/raw/oasis.rcd

- delete any “missing record references”


Eg. 
m1.0 0-16383



m1.1 0-16383

m1.2 0-16383

m1.3 0-5607,5641-5675

            Change last entry to m1.3 0-5675

 (this will prevent any dockside test records from being re-downloaded)

· resave and exit
Restart CRON job  (when ready for downloads to resume)
Edit /oasis/bin/oasis.cron  to disable the /oasis/test/ download and processing
Then restart the normal cronjob…

crontab /oasis/bin/oasis.cron 
Edit process script
- cd /oasis/bin

- vi process

- scroll do the doM1 or doM2 if block.

- Verify the instrument list for the new deployment matches above, plus ‘error’ directory
- verify the foreach year list will span the deployment, eg, 2008 2009.

- save and exit
