One-Stop Shopping for MBARI Upper Water Column Data : Upper Water Column Data This page last changed on Feb 03, 2009 by reiko. ## MBARI DATA ACCESS ### DATASETS
Platform | Access | Comments
Shipboard CTD | MS SQL | On Solstice, BOG database
Mooring | SSDS: SIAM Raw data access page GetOriginalDataServlet Explorer QC M0 (plot,data,netcdf) QC M1 (plot,data,netcdf) QC M2 (plot,data,netcdf) OASIS data archive (web) Live Access Server Real time, netcdf from DODS/SSDS Loboviz CIMT web pages (http) CIMT dods access | # http://new-ssds.mbari.org:8080/ssds/siamRawDataStep1.jsp http://new-ssds.mbari.org:8080/servlet/GetOriginalDataServlet http://new-ssds.mbari.org:8080/ssds/ http://dods.mbari.org/data/ssdsdata/deployments/m0/current_qcPlots.html http://dods.mbari.org/data/ssdsdata/deployments/m1/current_qcPlots.html http://dods.mbari.org/data/ssdsdata/deployments/m2/current_qcPlots.html http://dods.mbari.org:8085/mbariMoos/ncarchive.jsp http://dods.mbari.org/lasOASIS/ Real time current deployment: http://dods.mbari.org/cgi-bin/nph-nc/data/ssdsdata/deployments/m0/200706/m0_ctd0001_20070621_original.nc.html http://dods.mbari.org/cgi-bin/nph-nc/data/ssdsdata/deployments/ http://www.mbari.org/lobo/loboviz.htm http://new-ssds.mbari.org:8080/cimt/cimt.jsphttp://dods.mbari.org/cgi-bin/nph-nc/data/ssdsdata/deployments/#
AUVCTD | SSDS: Files on Tornado Web Mission Logs (http) Mission Logs (dods) Netcdf files (http) Netcdf files (dods) Ryan Lab processed files (http, netcdf, mat, images, odv, logs) Ryan Lab processed files (dods) | Tornado/auvctd Netcdf, mat, odv files http://dods.mbari.org/data/auvctd/surveys/ http://new-ssds.mbari.org/auvctd/missionlogs http://dods.mbari.org/cgi-bin/nph-nc/data/auvctd/missionlogs/ http://new-ssds.mbari.org/ssdsdata/ssds/generated/netcdf/files/ssds.shore.mbari.org/auvctd/missionlogs/ http://dods.mbari.org/cgi-bin/nph-nc/data/ssdsdata/ssds/generated/netcdf/files/ssds.shore.mbari.org/auvctd/missionlogs/ http://new-ssds.mbari.org/auvctd/surveys/2008/netcdf/http://dods.mbari.org/cgi-bin/nph-nc/data/auvctd/surveys/#
ROV-CTD | Samples DB, web access Web ARCHIVES | http://mww.mbari.org/samplesDB/queries/ http://search.mbari.org/ARCHIVE/rovctd/
Glider 014 | Web access via SPRAY data page | Line 67 MontereyBay (Scripps: http://spray.ucsd.edu/cgi-bin/archive_init.pl?start_archive=ARCHIVE+DATA)
NOEP | NOEP Web MS SQL | On FOG, BLS, Market, |
### PLATFORMS
Platform | Resolution | Location | Depths | Profiles
Ship (Time series) | Monthly | C1, M0, M1, M2 | Surface and profiles | Discrete bottle depths, profiles in meter bins
Ship (SECRET) | Quarterly | CalCOFI Stations | Surface and profiles | Discrete bottle depths, profiles in meter bins
AUV | Monthly | Various MontereyBay | Surface and profiles | Profiles in meters; yoyo surveys
ROV | Mission | Various MontereyBay | Surface and profiles | Various depths
Glider | Mission | CalCOFI Line 67 | Surface and profiles | Yoyo surveys
Mooring | 10 minute, hourly, daily | M0, M1, M2 | Surface and profiles | Discrete depths 0, 10, 20, 40, 60, 80, 100, 150, 200, 250, 300m |
### SAMPLES
Parameter | Platform
| Ship | Mooring | AUVCTD | ROV | Glider
Date Range | Mar 1989-present | Mar 1989-present | Apr 2003 -present | Oct 1988 - present | Apr 2007 - present
Frequency | Time series: Monthly SECRET: Quarterly (Line 67) | 10 min, hourly, daily | Missions occur monthly | Missions at irregular intervals | Missions quarterly duration 90 days
Type | CTD Bottle, Profiling | Surface CTD at fixed depths | Yo-yo surveys | Survey follows the ROV | Yo-yo surveys
Depth | Bottle 0,5,10,15,30,40, 60,80,100,150,200m Profiling 0-200 (1 m increments) | M0: 0, 10, 20, 40, 55m M1: 0,10,20,40,60,80, 100,150,200,250,300m M2: 0,10,20,40,60,80, 100,150,200,250,300m | 0-200m | Irregular depths | 0-200 m (5 m increments)
Location(map) | C1, Mooring1, Mooring2, CalCOFI Line 67 | M0 M1 M2 | CalCOFI Line 67 | Various locations in MontereyBay | CalCOFI Line 67
Temperature | Ship | Mooring | AUVCTD | ROV | Glider
Conductivity | Ship | Mooring |  |  |
Salinity | Ship | Mooring | AUVCTD | ROV | Glider
Transmissivity | Ship |  |  | ROV |
Oxygen | Ship | Mooring? Optode? surface | AUVCTD | ROV |
Fluorescence | Ship | Mooring, surface | AUVCTD |  | Glider
Density | Ship |  |  |  |
Nitrate | Ship |  | AUVCTD |  |
Bioluminescence |  |  | AUVCTD |  |
BBP at 676 & 470 |  |  | AUVCTD |  |
Metsys |  | Mooring, surface |  |  |
Air Temperature |  | Mooring, surface |  |  |
Winds (speed, direction) |  | Mooring, surface |  |  |
PCO2 |  |  |  |  |
ADCP |  | Mooring, surface |  |  |
PRR |  | Mooring, surface |  |  |  |

Document generated by Confluence on Feb 04, 2026 08:40