Support Engineering Group : Ventana ROV Control PC RHEL5 Linux Upgrade This page last changed on Sep 24, 2009 by kgomes. Experiment to determine issues upgrading older Pentium III PC from Red Hat 7 to RHEL5 Using the 'Simulator' duplicate PC (different motherboard than on Pt. Lobos) Using RHEL5 recovery disk and network (FTP) install. First problem, found that not enough memory (64M) was on the mother board. Found an old memory in Don's Legacy bin (PC133 ECC). ifconfig -a (or on windows ipconfig /all) 134.89.12.69 (Palmer) \ 255.255.254.0 Gateway: 134.89.32.1

Document generated by Confluence on Feb 03, 2026 16:22