Support Engineering Group : FOCE DC-DC Converter assembly notes This page last changed on Sep 24, 2009 by kgomes. ## ## DC-DC converter assembly notes ## BOM Corrections: 1. C99, BOM states 10nF in PART field. It should be 22nF. 2. JP8, JP9, JP12, JP13, JP18: Manuf PN field has a typo. The correct PN should be 87215-1. 3. JP16: Manuf PN field has a typo. The correct PN should be 87215-1. 4. J24. Manufacturer PN is obsolete. This affects the layout footprint. Possible substitue parts do not match the layout footprint. SUB PN's are Molex 500998-0900 or Molex 67913-8008. 5. R35, R36, R50, R52: BOM specifies a zero OHM resistor in the PART field. This is due to a change in the schematic. The Manuf PN and Supplier PN fields need to update to PANASONIC ERJ-8GEY0R000V. 6. R84, R 86, R88, R91 Change 511 to 510 in PART field.

Document generated by Confluence on Feb 03, 2026 16:22