500049 Video Annotation and Reference System : Solstice This page last changed on Jan 10, 2012 by brian. ## About Solstice Solistice hosts the MS SQL Server for the Shore VARS database ### About Oxygen From [~rich]: Primary is o2 (seabird sensor) Secondary is o2alt (optode) Flags... 0=bad, 1=suspect, 2='loaded by perl', 3='actually looked at and blessed by ctd/science tech',4= winklers were run etc (don't expect to see any of these "yet"') Note that flags are a per-record basis, when data is loaded and o2 computed from raw... it will typically set some flags to 0 when 'out-of-range' or if p,t,s is bad etc....(since needs p,t,s in the O2 formula...)

Document generated by Confluence on Feb 03, 2026 12:59