500049 Video Annotation and Reference System : VARS-WF This page last changed on Aug 06, 2015 by brian. ## About vars-wf.wf.mbari.org VARS-WF is the computer on the R/V Western Flyer used for running VARS VARS is launched via Java Web Start on VARS-WF. Each application has a correspoding desktop shortcut and start menu item; they should appear as reqular applications to the users and no network connection is needed to launch them. The location of the web start applications are C:\Program Files\VARS\webstart. The applications here can be updated by following the build instructions for the 'vars-mbari' module on moonjelly, then executing the modules build file with 'ant deploy.jnlp.wf' ## Timecode source VARS on the flyer gets timecode and time via UDP from navproc.wf.mbari.org. Beta timecode can be fetched on port 9000. HD timecode is on port 9001. ## NTP From [~sheldon]: vars-wf is configured to synchronize with the following: Western Flyer: time-wf1 (134.89.20.17), time-wf2 (Unused), time-wf3 (134.89.21.5), time-wf4 (134.89.21.6) ntp.conf
    server time-wf1
    server time-wf2
    server time-wf3
    server time-wf4

Document generated by Confluence on Feb 03, 2026 12:59