LEFT HANDED TOOLING                                          X OFFSET VALUE

RRL-087-8 GRV TOOL                                                             X                       

ITL-230750 THREAD TOOL                                                    X 
CHUCKING MODE  /  MDI MODE NEEDED

M28 = INTERNAL

M27 = EXTERNAL
TOOL #1 (IF STILL MOUNTED IN MACHINE)

X4.5900  Z0.0000  (WITH .030 RADIUS INSERT)
PART OFF TOOL (IF STILL MOUNTED IN HOLDER)

1.00 CORODRILL 880                                                   X OFFSET VALUE

WHEN USED FOR ROUGHING ID                                   X-1.000

.750 CORODRILL 880                                                       

WHEN USED FOR ROUGHING ID                                   X-  .750
WORK SHIFT ADJUSTMENTS   +.010    INPUT+   

(REMOVES MORE MATERIAL FROM FACE OF PART)

DISTANCE TO GO IN “X” 

THE VALUE IS DOUBLE THE REAL AMOUNT TO TRAVEL IN X
INTERNAL TOOL                            MIN. BORE           X OFFSET VALUE
T-320-750                                              .320                          X               

T-360-1000                                            .360                          X

T-490-1000                                            .490                          X

T-490-1500                                            .490                          X

T-490-2000                                            .490                          X

T-180-750                                              .180                          X

T-230-750                                              .230                          X

R-156-16                                                .500                          X
MG-50-063-1000                                   .500                          X 

MG-37-039-500                                    .375                           X

MG-37-069-500                                    .375                           X

MG-50-125-1000                                  .500                           X

MG-31-094-1000                                  .375                           X

G-030-4                                                  .250                          X

G-062-8                                                 .375                           X

B-230-800                                             .230                           X
B-180-500                                             .180                           X

B-160-250                                             .160                          X
B-320-1000



  .320                           X

B-200-500                                             .200                           X
B-490-1250                                           .490                           X

B-290-750                                             .290                           X        

FACE GROOVE TOOLS                                                 X OFFSET VALUE
SANDVIK  CXS-A0750-06      .098 WIDE                          X.0045
SANDVIK  CXS-A0750-06      .079 WIDE                          X
SANDVIK  CXS-A0750-06      .069 WIDE                          X

PH HORN (BU105.0750.02)    .099 WIDE                           X

PH HORN (BU114.ST06.00)    .094 WIDE                           X
HOME MADE TOOL               .250 WIDE                           X

HOME MADE TOOL               .187 WIDE                           X
HOME MADE FACE GRV      .187 WIDE                           X

SANDVIK MBS4-151.2 i-055B-25  .122 WIDE                   X
SANDVIK MBS4-151.2 i-055B-25  1/8 RADIUS                X

INTERNAL TOOLS SFGR-250-375                                     X

THINBIT DGPC20133402        .078 WIDE                          X

THINBITLFT58R                      .080 WIDE                          X
SANDVIK 570-32R123G18B130B   ,125 WIDE                  X

BORING BARS                                                                X OFFSET VALUE

1.000-S12S         SCLCR-3M                                                 X     

.500-S06M          SCLCR-2                                                    X

.750-S10R           SCLCR-3                                                    X

.625-A08M         SCLCR-2                                                     X-.6125
GHIR  19-3                                                                             X

1.000 -A16T       SCLCR3                                                      X

1.000 – A570-2C D16 07-25                                                  X
ID GROOVE TOOLS

SANDVIK  RAG123H039-20B                                           X
SANDVIK  MBE0625-13-09 R      .079 WIDE                   X
SANDVIK  MBE0625-17-09 R      .119 WIDE                   X

SANDVIK  MBE0625-17-09 R      .037 WIDE                   X
ID THREADING TOOLS

SANDVIK R166.4K-D10-3                                                  X

SMALL ID SIR 0310 K08U                                                 X
CSX-04TH070MM-4215R 1025                                          X   

CSX-06TH100VM-6215R  1025                                          X
