ROMI CNC LATHE TOOLS
TOOLS ON ROMI OFFSET PARAMETER PAGE ARE SET UP AS FOLLOWS
USE THESE TOOL #’S AND TOOL TYPES WHEN PROGRAMING ROMI LATHE

T1    OD TURNING   ROUGHING AND / OR FINISHING

T2    OD TURNING   ROUGHING AND / OR FINISHING

T3    DRILLING ID

T4    DRILLING ID

T5    TAP ID

T6     OD GROOVING

T7     OD THREADING

T8    ID  BORING

T9    ID GROOVING

T10   FACE GROOVING

T11  ID GROOVING

T12  PART OFF TOOL
CLAMP OD OF PART   M81

CLAMP ID OF PART    M82

CLAMP PART IN DIRECTION NEEDED

GO TO MDA

TYPE IN

G291

M81 / M82 (WHATEVER IS NEEDED)

PUSH CYCLE START

ALARM SOUNDS

HIT RESET

CHECK CLAMPING FOR CORRECT DIRECTION

T1  X 5.8135    Z 1.8572  .015 R     (IF NOT REMOVED FROM HOLDER)

